# Static Call Graph for image .\STM3210B-EVAL\STM3210B-EVAL.axf

#<CALLGRAPH># ARM Linker, 4.1 [Build 561]: Last Updated: Thu Apr 14 21:53:38 2011

### Maximum Stack Usage = 0 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(i.BusFault_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(i.DebugMon_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - EP1_IN_Callback from usb_endp.o(i.EP1_IN_Callback) referenced 2 times from usb_istr.o(.data)
  - EP3_OUT_Callback from usb_endp.o(i.EP3_OUT_Callback) referenced 2 times from usb_istr.o(.data)
  - EXTI0_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - HardFault_Handler from stm32f10x_it.o(i.HardFault_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(i.MemManage_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - NMI_Handler from stm32f10x_it.o(i.NMI_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - NOP_Process from usb_core.o(i.NOP_Process) referenced 24 times from usb_istr.o(.data)
  - NOP_Process from usb_core.o(i.NOP_Process) referenced 14 times from usb_prop.o(.data)
  - PVD_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - PendSV_Handler from stm32f10x_it.o(i.PendSV_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - RTC_IRQHandler from stm32f10x_it.o(i.RTC_IRQHandler) referenced from startup_stm32f10x_md.o(RESET)
  - Reset_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SVC_Handler from stm32f10x_it.o(i.SVC_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - Standard_GetConfiguration from usb_core.o(i.Standard_GetConfiguration) referenced from usb_core.o(i.Data_Setup0)
  - Standard_GetInterface from usb_core.o(i.Standard_GetInterface) referenced from usb_core.o(i.Data_Setup0)
  - Standard_GetStatus from usb_core.o(i.Standard_GetStatus) referenced from usb_core.o(i.Data_Setup0)
  - SysTick_Handler from stm32f10x_it.o(i.SysTick_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - SystemInit from system_stm32f10x.o(i.SystemInit) referenced from startup_stm32f10x_md.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USART1_IRQHandler from stm32f10x_it.o(i.USART1_IRQHandler) referenced from startup_stm32f10x_md.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from stm32f10x_it.o(i.USB_LP_CAN1_RX0_IRQHandler) referenced from startup_stm32f10x_md.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(i.UsageFault_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - Virtual_Com_Port_Data_Setup from usb_prop.o(i.Virtual_Com_Port_Data_Setup) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_GetConfigDescriptor from usb_prop.o(i.Virtual_Com_Port_GetConfigDescriptor) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_GetDeviceDescriptor from usb_prop.o(i.Virtual_Com_Port_GetDeviceDescriptor) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_GetLineCoding from usb_prop.o(i.Virtual_Com_Port_GetLineCoding) referenced from usb_prop.o(i.Virtual_Com_Port_Data_Setup)
  - Virtual_Com_Port_GetStringDescriptor from usb_prop.o(i.Virtual_Com_Port_GetStringDescriptor) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_Get_Interface_Setting from usb_prop.o(i.Virtual_Com_Port_Get_Interface_Setting) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_NoData_Setup from usb_prop.o(i.Virtual_Com_Port_NoData_Setup) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_Reset from usb_prop.o(i.Virtual_Com_Port_Reset) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_SetConfiguration from usb_prop.o(i.Virtual_Com_Port_SetConfiguration) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_SetDeviceAddress from usb_prop.o(i.Virtual_Com_Port_SetDeviceAddress) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_SetLineCoding from usb_prop.o(i.Virtual_Com_Port_SetLineCoding) referenced from usb_prop.o(i.Virtual_Com_Port_Data_Setup)
  - Virtual_Com_Port_Status_In from usb_prop.o(i.Virtual_Com_Port_Status_In) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_Status_Out from usb_prop.o(i.Virtual_Com_Port_Status_Out) referenced 2 times from usb_prop.o(.data)
  - Virtual_Com_Port_init from usb_prop.o(i.Virtual_Com_Port_init) referenced 2 times from usb_prop.o(.data)
  - WWDG_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f10x_md.o(.text)
  - fputc from usb_init.o(i.fputc) referenced from printf1.o(i.__0printf$1)
  - main from main.o(i.main) referenced from entry7.o(.ARM.Collect$$$$00000007)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size 0 bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(.text)

  _main_scatterload (Thumb, 0 bytes, Stack size 0 bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size 0 bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  __aeabi_dadd (Thumb, 318 bytes, Stack size 0 bytes, dadd.o(.text))
  [Calls]

  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_round
  - >> _double_epilogue
  [Called By]
  - >> __aeabi_drsub
  - >> Count_Temperature
  - >> __aeabi_dsub

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text))
  [Calls]

  - >> __aeabi_dadd
  [Called By]
  - >> Count_Temperature

  __aeabi_dmul (Thumb, 226 bytes, Stack size 0 bytes, dmul.o(.text))
  [Calls]

  - >> _double_epilogue
  [Called By]
  - >> Count_Temperature

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 0 bytes, ddiv.o(.text))
  [Calls]

  - >> _double_round
  [Called By]
  - >> Count_Temperature

  __aeabi_ui2d (Thumb, 26 bytes, Stack size 0 bytes, dfltui.o(.text))
  [Calls]

  - >> _double_epilogue
  [Called By]
  - >> Count_Temperature

  __aeabi_d2uiz (Thumb, 46 bytes, Stack size 0 bytes, dfixui.o(.text))
  [Calls]

  - >> __aeabi_llsr
  [Called By]
  - >> Count_Temperature

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 0 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_dadd
  - >> _double_epilogue

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_d2uiz
  - >> _double_epilogue

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text))
  [Called By]

  - >> __aeabi_dadd

  _double_round (Thumb, 26 bytes, Stack size 0 bytes, depilogue.o(.text))
  [Called By]

  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> _double_epilogue

  _double_epilogue (Thumb, 168 bytes, Stack size 0 bytes, depilogue.o(.text))
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> _double_round
  [Called By]
  - >> __aeabi_ui2d
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  ADC_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_Cmd))
  [Called By]

  - >> ADC_Configuration

  ADC_Configuration (Thumb, 124 bytes, Stack size 0 bytes, main.o(i.ADC_Configuration))
  [Calls]

  - >> ADC_TempSensorVrefintCmd
  - >> ADC_StartCalibration
  - >> ADC_SoftwareStartConvCmd
  - >> ADC_ResetCalibration
  - >> ADC_RegularChannelConfig
  - >> ADC_Init
  - >> ADC_GetResetCalibrationStatus
  - >> ADC_GetCalibrationStatus
  - >> ADC_DMACmd
  - >> ADC_Cmd
  [Called By]
  - >> main

  ADC_DMACmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_DMACmd))
  [Called By]

  - >> ADC_Configuration

  ADC_Filter (Thumb, 42 bytes, Stack size 0 bytes, main.o(i.ADC_Filter))
  [Calls]

  - >> Delay
  [Called By]
  - >> Count_Temperature

  ADC_GetCalibrationStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_GetCalibrationStatus))
  [Called By]

  - >> ADC_Configuration

  ADC_GetResetCalibrationStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_GetResetCalibrationStatus))
  [Called By]

  - >> ADC_Configuration

  ADC_Init (Thumb, 62 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_Init))
  [Called By]

  - >> ADC_Configuration

  ADC_RegularChannelConfig (Thumb, 116 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_RegularChannelConfig))
  [Called By]

  - >> ADC_Configuration

  ADC_ResetCalibration (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_ResetCalibration))
  [Called By]

  - >> ADC_Configuration

  ADC_SoftwareStartConvCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_SoftwareStartConvCmd))
  [Called By]

  - >> ADC_Configuration

  ADC_StartCalibration (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_StartCalibration))
  [Called By]

  - >> ADC_Configuration

  ADC_TempSensorVrefintCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_TempSensorVrefintCmd))
  [Called By]

  - >> ADC_Configuration

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  ByteSwap (Thumb, 12 bytes, Stack size 0 bytes, usb_regs.o(i.ByteSwap))
  [Called By]

  - >> Setup0_Process

  CTR_LP (Thumb, 612 bytes, Stack size 0 bytes, usb_int.o(i.CTR_LP))
  [Calls]

  - >> Setup0_Process
  - >> Out0_Process
  - >> In0_Process
  [Called By]
  - >> USB_Istr

  ClearDTOG_RX (Thumb, 52 bytes, Stack size 0 bytes, usb_regs.o(i.ClearDTOG_RX))
  [Called By]

  - >> Standard_ClearFeature

  ClearDTOG_TX (Thumb, 52 bytes, Stack size 0 bytes, usb_regs.o(i.ClearDTOG_TX))
  [Called By]

  - >> Standard_ClearFeature

  Clear_Status_Out (Thumb, 36 bytes, Stack size 0 bytes, usb_regs.o(i.Clear_Status_Out))
  [Called By]

  - >> Virtual_Com_Port_Reset

  Count_Temperature (Thumb, 110 bytes, Stack size 0 bytes, main.o(i.Count_Temperature))
  [Calls]

  - >> __aeabi_ui2d
  - >> __aeabi_drsub
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2uiz
  - >> ADC_Filter
  - >> __2printf
  [Called By]
  - >> main

  DMA_Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_dma.o(i.DMA_Cmd))
  [Called By]

  - >> DMA_Configuration

  DMA_Configuration (Thumb, 74 bytes, Stack size 0 bytes, main.o(i.DMA_Configuration))
  [Calls]

  - >> DMA_Init
  - >> DMA_DeInit
  - >> DMA_Cmd
  [Called By]
  - >> main

  DMA_DeInit (Thumb, 228 bytes, Stack size 0 bytes, stm32f10x_dma.o(i.DMA_DeInit))
  [Called By]

  - >> DMA_Configuration

  DMA_Init (Thumb, 58 bytes, Stack size 0 bytes, stm32f10x_dma.o(i.DMA_Init))
  [Called By]

  - >> DMA_Configuration

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  Delay (Thumb, 10 bytes, Stack size 0 bytes, main.o(i.Delay))
  [Called By]

  - >> ADC_Filter

  EP1_IN_Callback (Thumb, 122 bytes, Stack size 0 bytes, usb_endp.o(i.EP1_IN_Callback))
  [Calls]

  - >> UserToPMABufferCopy
  - >> SetEPTxValid
  - >> SetEPTxCount
  [Address Reference Count : 1]
  - usb_istr.o(.data)

  EP3_OUT_Callback (Thumb, 40 bytes, Stack size 0 bytes, usb_endp.o(i.EP3_OUT_Callback))
  [Calls]

  - >> USB_SIL_Read
  - >> SetEPRxValid
  - >> USB_To_USART_Send_Data
  [Address Reference Count : 1]
  - usb_istr.o(.data)

  FLASH_PrefetchBufferCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_PrefetchBufferCmd))
  [Called By]

  - >> Set_System

  FLASH_SetLatency (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_SetLatency))
  [Called By]

  - >> Set_System

  GPIO_Configuration (Thumb, 32 bytes, Stack size 0 bytes, main.o(i.GPIO_Configuration))
  [Calls]

  - >> GPIO_Init
  [Called By]
  - >> main

  GPIO_Init (Thumb, 164 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_Init))
  [Called By]

  - >> GPIO_Configuration
  - >> STM_EVAL_COMInit
  - >> Set_System

  GPIO_PinRemapConfig (Thumb, 82 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_PinRemapConfig))
  [Called By]

  - >> STM_EVAL_COMInit

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ReadInputDataBit))
  [Called By]

  - >> main

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ResetBits))
  [Called By]

  - >> USB_Cable_Config

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_SetBits))
  [Called By]

  - >> USB_Cable_Config

  GetEPRxAddr (Thumb, 26 bytes, Stack size 0 bytes, usb_regs.o(i.GetEPRxAddr))
  [Called By]

  - >> DataStageOut
  - >> USB_SIL_Read

  GetEPRxCount (Thumb, 28 bytes, Stack size 0 bytes, usb_regs.o(i.GetEPRxCount))
  [Called By]

  - >> USB_SIL_Read

  GetEPTxAddr (Thumb, 22 bytes, Stack size 0 bytes, usb_regs.o(i.GetEPTxAddr))
  [Called By]

  - >> DataStageIn

  Get_SerialNum (Thumb, 44 bytes, Stack size 0 bytes, hw_config.o(i.Get_SerialNum))
  [Calls]

  - >> IntToUnicode
  [Called By]
  - >> Virtual_Com_Port_init

  Handle_USBAsynchXfer (Thumb, 192 bytes, Stack size 0 bytes, hw_config.o(i.Handle_USBAsynchXfer))
  [Calls]

  - >> UserToPMABufferCopy
  - >> SetEPTxValid
  - >> SetEPTxCount
  [Called By]
  - >> SOF_Callback

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  In0_Process (Thumb, 98 bytes, Stack size 0 bytes, usb_core.o(i.In0_Process))
  [Calls]

  - >> Post0_Process
  - >> DataStageIn
  - >> SetDeviceAddress
  [Called By]
  - >> CTR_LP

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  NOP_Process (Thumb, 2 bytes, Stack size 0 bytes, usb_core.o(i.NOP_Process))
  [Address Reference Count : 2]

  - usb_prop.o(.data)
  - usb_istr.o(.data)

  NVIC_Init (Thumb, 92 bytes, Stack size 0 bytes, misc.o(i.NVIC_Init))
  [Called By]

  - >> USB_Interrupts_Config

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(i.NVIC_PriorityGroupConfig))
  [Called By]

  - >> USB_Interrupts_Config

  NVIC_SetVectorTable (Thumb, 12 bytes, Stack size 0 bytes, misc.o(i.NVIC_SetVectorTable))
  [Called By]

  - >> USB_Interrupts_Config

  Out0_Process (Thumb, 70 bytes, Stack size 0 bytes, usb_core.o(i.Out0_Process))
  [Calls]

  - >> Post0_Process
  - >> DataStageOut
  [Called By]
  - >> CTR_LP

  PMAToUserBufferCopy (Thumb, 32 bytes, Stack size 0 bytes, usb_mem.o(i.PMAToUserBufferCopy))
  [Called By]

  - >> DataStageOut
  - >> USB_SIL_Read

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  Post0_Process (Thumb, 56 bytes, Stack size 0 bytes, usb_core.o(i.Post0_Process))
  [Calls]

  - >> SetEPRxCount
  [Called By]
  - >> Setup0_Process
  - >> Out0_Process
  - >> In0_Process

  PowerOn (Thumb, 64 bytes, Stack size 0 bytes, usb_pwr.o(i.PowerOn))
  [Calls]

  - >> USB_Cable_Config
  [Called By]
  - >> Virtual_Com_Port_init

  RCC_AHBPeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_AHBPeriphClockCmd))
  [Called By]

  - >> RCC_Configuration

  RCC_APB1PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> STM_EVAL_COMInit
  - >> Set_USBClock

  RCC_APB2PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> RCC_Configuration
  - >> STM_EVAL_COMInit
  - >> Set_System

  RCC_Configuration (Thumb, 28 bytes, Stack size 0 bytes, main.o(i.RCC_Configuration))
  [Calls]

  - >> RCC_AHBPeriphClockCmd
  - >> RCC_APB2PeriphClockCmd
  [Called By]
  - >> main

  RCC_DeInit (Thumb, 50 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_DeInit))
  [Called By]

  - >> Set_System

  RCC_GetClocksFreq (Thumb, 136 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_GetClocksFreq))
  [Called By]

  - >> USART_Init

  RCC_GetFlagStatus (Thumb, 44 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_GetFlagStatus))
  [Called By]

  - >> RCC_WaitForHSEStartUp
  - >> Set_System

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_GetSYSCLKSource))
  [Called By]

  - >> Set_System

  RCC_HCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_HCLKConfig))
  [Called By]

  - >> Set_System

  RCC_HSEConfig (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_HSEConfig))
  [Called By]

  - >> Set_System

  RCC_PCLK1Config (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PCLK1Config))
  [Called By]

  - >> Set_System

  RCC_PCLK2Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PCLK2Config))
  [Called By]

  - >> Set_System

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PLLCmd))
  [Called By]

  - >> Set_System

  RCC_PLLConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PLLConfig))
  [Called By]

  - >> Set_System

  RCC_SYSCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_SYSCLKConfig))
  [Called By]

  - >> Set_System

  RCC_USBCLKConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_USBCLKConfig))
  [Called By]

  - >> Set_USBClock

  RCC_WaitForHSEStartUp (Thumb, 38 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_WaitForHSEStartUp))
  [Calls]

  - >> RCC_GetFlagStatus
  [Called By]
  - >> Set_System

  RTC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.RTC_IRQHandler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SOF_Callback (Thumb, 38 bytes, Stack size 0 bytes, usb_endp.o(i.SOF_Callback))
  [Calls]

  - >> Handle_USBAsynchXfer
  [Called By]
  - >> USB_Istr

  STM_EVAL_COMInit (Thumb, 154 bytes, Stack size 0 bytes, stm32_eval.o(i.STM_EVAL_COMInit))
  [Calls]

  - >> USART_Init
  - >> USART_Cmd
  - >> GPIO_PinRemapConfig
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> USART_Config_Default
  - >> USART_Config

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SetBTABLE (Thumb, 12 bytes, Stack size 0 bytes, usb_regs.o(i.SetBTABLE))
  [Called By]

  - >> Virtual_Com_Port_Reset

  SetDeviceAddress (Thumb, 70 bytes, Stack size 0 bytes, usb_core.o(i.SetDeviceAddress))
  [Called By]

  - >> In0_Process
  - >> Virtual_Com_Port_Reset

  SetEPRxAddr (Thumb, 28 bytes, Stack size 0 bytes, usb_regs.o(i.SetEPRxAddr))
  [Called By]

  - >> Virtual_Com_Port_Reset

  SetEPRxCount (Thumb, 70 bytes, Stack size 0 bytes, usb_regs.o(i.SetEPRxCount))
  [Called By]

  - >> Standard_ClearFeature
  - >> Post0_Process
  - >> Virtual_Com_Port_Reset

  SetEPRxStatus (Thumb, 62 bytes, Stack size 0 bytes, usb_regs.o(i.SetEPRxStatus))
  [Called By]

  - >> Virtual_Com_Port_Reset

  SetEPRxValid (Thumb, 48 bytes, Stack size 0 bytes, usb_regs.o(i.SetEPRxValid))
  [Called By]

  - >> Virtual_Com_Port_Reset
  - >> EP3_OUT_Callback

  SetEPTxAddr (Thumb, 24 bytes, Stack size 0 bytes, usb_regs.o(i.SetEPTxAddr))
  [Called By]

  - >> Virtual_Com_Port_Reset

  SetEPTxCount (Thumb, 22 bytes, Stack size 0 bytes, usb_regs.o(i.SetEPTxCount))
  [Called By]

  - >> DataStageOut
  - >> DataStageIn
  - >> EP1_IN_Callback
  - >> Handle_USBAsynchXfer

  SetEPTxStatus (Thumb, 62 bytes, Stack size 0 bytes, usb_regs.o(i.SetEPTxStatus))
  [Called By]

  - >> Standard_ClearFeature
  - >> Virtual_Com_Port_Reset

  SetEPTxValid (Thumb, 48 bytes, Stack size 0 bytes, usb_regs.o(i.SetEPTxValid))
  [Called By]

  - >> EP1_IN_Callback
  - >> Handle_USBAsynchXfer

  SetEPType (Thumb, 32 bytes, Stack size 0 bytes, usb_regs.o(i.SetEPType))
  [Called By]

  - >> Virtual_Com_Port_Reset

  Set_System (Thumb, 164 bytes, Stack size 0 bytes, hw_config.o(i.Set_System))
  [Calls]

  - >> USB_Init
  - >> RCC_WaitForHSEStartUp
  - >> RCC_SYSCLKConfig
  - >> RCC_PLLConfig
  - >> RCC_PLLCmd
  - >> RCC_PCLK2Config
  - >> RCC_PCLK1Config
  - >> RCC_HSEConfig
  - >> RCC_HCLKConfig
  - >> RCC_GetSYSCLKSource
  - >> RCC_GetFlagStatus
  - >> RCC_DeInit
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> FLASH_SetLatency
  - >> FLASH_PrefetchBufferCmd
  - >> USB_Interrupts_Config
  - >> Set_USBClock
  [Called By]
  - >> main

  Set_USBClock (Thumb, 18 bytes, Stack size 0 bytes, hw_config.o(i.Set_USBClock))
  [Calls]

  - >> RCC_USBCLKConfig
  - >> RCC_APB1PeriphClockCmd
  [Called By]
  - >> Set_System

  Setup0_Process (Thumb, 172 bytes, Stack size 0 bytes, usb_core.o(i.Setup0_Process))
  [Calls]

  - >> ByteSwap
  - >> Post0_Process
  - >> NoData_Setup0
  - >> Data_Setup0
  [Called By]
  - >> CTR_LP

  Standard_ClearFeature (Thumb, 346 bytes, Stack size 0 bytes, usb_core.o(i.Standard_ClearFeature))
  [Calls]

  - >> ClearDTOG_TX
  - >> ClearDTOG_RX
  - >> SetEPTxStatus
  - >> SetEPRxCount
  [Called By]
  - >> NoData_Setup0

  Standard_GetConfiguration (Thumb, 34 bytes, Stack size 0 bytes, usb_core.o(i.Standard_GetConfiguration))
  [Address Reference Count : 1]

  - usb_core.o(i.Data_Setup0)

  Standard_GetDescriptorData (Thumb, 32 bytes, Stack size 0 bytes, usb_core.o(i.Standard_GetDescriptorData))
  [Called By]

  - >> Virtual_Com_Port_GetStringDescriptor
  - >> Virtual_Com_Port_GetDeviceDescriptor
  - >> Virtual_Com_Port_GetConfigDescriptor

  Standard_GetInterface (Thumb, 34 bytes, Stack size 0 bytes, usb_core.o(i.Standard_GetInterface))
  [Address Reference Count : 1]

  - usb_core.o(i.Data_Setup0)

  Standard_GetStatus (Thumb, 238 bytes, Stack size 0 bytes, usb_core.o(i.Standard_GetStatus))
  [Address Reference Count : 1]

  - usb_core.o(i.Data_Setup0)

  Standard_SetConfiguration (Thumb, 60 bytes, Stack size 0 bytes, usb_core.o(i.Standard_SetConfiguration))
  [Called By]

  - >> NoData_Setup0

  Standard_SetDeviceFeature (Thumb, 30 bytes, Stack size 0 bytes, usb_core.o(i.Standard_SetDeviceFeature))
  [Called By]

  - >> NoData_Setup0

  Standard_SetEndPointFeature (Thumb, 196 bytes, Stack size 0 bytes, usb_core.o(i.Standard_SetEndPointFeature))
  [Called By]

  - >> NoData_Setup0

  Standard_SetInterface (Thumb, 96 bytes, Stack size 0 bytes, usb_core.o(i.Standard_SetInterface))
  [Called By]

  - >> NoData_Setup0

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SystemInit (Thumb, 70 bytes, Stack size 0 bytes, system_stm32f10x.o(i.SystemInit))
  [Calls]

  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(.text)

  USART1_IRQHandler (Thumb, 36 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USART1_IRQHandler))
  [Calls]

  - >> USART_GetITStatus
  - >> USART_ReceiveData
  - >> USART_GetFlagStatus
  - >> USART_To_USB_Send_Data
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  USART_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_Cmd))
  [Called By]

  - >> STM_EVAL_COMInit

  USART_Config (Thumb, 192 bytes, Stack size 0 bytes, hw_config.o(i.USART_Config))
  [Calls]

  - >> STM_EVAL_COMInit
  - >> USART_Config_Default
  [Called By]
  - >> Virtual_Com_Port_Status_In

  USART_Config_Default (Thumb, 44 bytes, Stack size 0 bytes, hw_config.o(i.USART_Config_Default))
  [Calls]

  - >> USART_ITConfig
  - >> STM_EVAL_COMInit
  [Called By]
  - >> Virtual_Com_Port_init
  - >> USART_Config

  USART_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_GetFlagStatus))
  [Called By]

  - >> USART1_IRQHandler
  - >> USB_To_USART_Send_Data

  USART_GetITStatus (Thumb, 62 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_GetITStatus))
  [Called By]

  - >> USART1_IRQHandler

  USART_ITConfig (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_ITConfig))
  [Called By]

  - >> USART_Config_Default

  USART_Init (Thumb, 176 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_Init))
  [Calls]

  - >> RCC_GetClocksFreq
  [Called By]
  - >> STM_EVAL_COMInit

  USART_ReceiveData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_ReceiveData))
  [Called By]

  - >> USART1_IRQHandler
  - >> USART_To_USB_Send_Data

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_SendData))
  [Called By]

  - >> USB_To_USART_Send_Data

  USART_To_USB_Send_Data (Thumb, 78 bytes, Stack size 0 bytes, hw_config.o(i.USART_To_USB_Send_Data))
  [Calls]

  - >> USART_ReceiveData
  [Called By]
  - >> USART1_IRQHandler

  USB_Cable_Config (Thumb, 30 bytes, Stack size 0 bytes, hw_config.o(i.USB_Cable_Config))
  [Calls]

  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> PowerOn

  USB_Init (Thumb, 36 bytes, Stack size 0 bytes, usb_init.o(i.USB_Init))
  [Called By]

  - >> Set_System

  USB_Interrupts_Config (Thumb, 68 bytes, Stack size 0 bytes, hw_config.o(i.USB_Interrupts_Config))
  [Calls]

  - >> NVIC_SetVectorTable
  - >> NVIC_PriorityGroupConfig
  - >> NVIC_Init
  [Called By]
  - >> Set_System

  USB_Istr (Thumb, 102 bytes, Stack size 0 bytes, usb_istr.o(i.USB_Istr))
  [Calls]

  - >> CTR_LP
  - >> SOF_Callback
  [Called By]
  - >> USB_LP_CAN1_RX0_IRQHandler

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USB_LP_CAN1_RX0_IRQHandler))
  [Calls]

  - >> USB_Istr
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  USB_SIL_Init (Thumb, 30 bytes, Stack size 0 bytes, usb_sil.o(i.USB_SIL_Init))
  [Called By]

  - >> Virtual_Com_Port_init

  USB_SIL_Read (Thumb, 46 bytes, Stack size 0 bytes, usb_sil.o(i.USB_SIL_Read))
  [Calls]

  - >> GetEPRxCount
  - >> PMAToUserBufferCopy
  - >> GetEPRxAddr
  [Called By]
  - >> EP3_OUT_Callback

  USB_To_USART_Send_Data (Thumb, 40 bytes, Stack size 0 bytes, hw_config.o(i.USB_To_USART_Send_Data))
  [Calls]

  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Called By]
  - >> EP3_OUT_Callback

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  UserToPMABufferCopy (Thumb, 52 bytes, Stack size 0 bytes, usb_mem.o(i.UserToPMABufferCopy))
  [Called By]

  - >> DataStageIn
  - >> EP1_IN_Callback
  - >> Handle_USBAsynchXfer

  Virtual_Com_Port_Data_Setup (Thumb, 82 bytes, Stack size 0 bytes, usb_prop.o(i.Virtual_Com_Port_Data_Setup))
  [Address Reference Count : 1]

  - usb_prop.o(.data)

  Virtual_Com_Port_GetConfigDescriptor (Thumb, 14 bytes, Stack size 0 bytes, usb_prop.o(i.Virtual_Com_Port_GetConfigDescriptor))
  [Calls]

  - >> Standard_GetDescriptorData
  [Address Reference Count : 1]
  - usb_prop.o(.data)

  Virtual_Com_Port_GetDeviceDescriptor (Thumb, 14 bytes, Stack size 0 bytes, usb_prop.o(i.Virtual_Com_Port_GetDeviceDescriptor))
  [Calls]

  - >> Standard_GetDescriptorData
  [Address Reference Count : 1]
  - usb_prop.o(.data)

  Virtual_Com_Port_GetLineCoding (Thumb, 20 bytes, Stack size 0 bytes, usb_prop.o(i.Virtual_Com_Port_GetLineCoding))
  [Address Reference Count : 1]

  - usb_prop.o(i.Virtual_Com_Port_Data_Setup)

  Virtual_Com_Port_GetStringDescriptor (Thumb, 32 bytes, Stack size 0 bytes, usb_prop.o(i.Virtual_Com_Port_GetStringDescriptor))
  [Calls]

  - >> Standard_GetDescriptorData
  [Address Reference Count : 1]
  - usb_prop.o(.data)

  Virtual_Com_Port_Get_Interface_Setting (Thumb, 22 bytes, Stack size 0 bytes, usb_prop.o(i.Virtual_Com_Port_Get_Interface_Setting))
  [Address Reference Count : 1]

  - usb_prop.o(.data)

  Virtual_Com_Port_NoData_Setup (Thumb, 36 bytes, Stack size 0 bytes, usb_prop.o(i.Virtual_Com_Port_NoData_Setup))
  [Address Reference Count : 1]

  - usb_prop.o(.data)

  Virtual_Com_Port_Reset (Thumb, 216 bytes, Stack size 0 bytes, usb_prop.o(i.Virtual_Com_Port_Reset))
  [Calls]

  - >> SetEPType
  - >> SetEPTxStatus
  - >> SetEPTxAddr
  - >> SetEPRxStatus
  - >> SetEPRxCount
  - >> SetEPRxAddr
  - >> SetDeviceAddress
  - >> SetBTABLE
  - >> Clear_Status_Out
  - >> SetEPRxValid
  [Address Reference Count : 1]
  - usb_prop.o(.data)

  Virtual_Com_Port_SetConfiguration (Thumb, 14 bytes, Stack size 0 bytes, usb_prop.o(i.Virtual_Com_Port_SetConfiguration))
  [Address Reference Count : 1]

  - usb_prop.o(.data)

  Virtual_Com_Port_SetDeviceAddress (Thumb, 8 bytes, Stack size 0 bytes, usb_prop.o(i.Virtual_Com_Port_SetDeviceAddress))
  [Address Reference Count : 1]

  - usb_prop.o(.data)

  Virtual_Com_Port_SetLineCoding (Thumb, 20 bytes, Stack size 0 bytes, usb_prop.o(i.Virtual_Com_Port_SetLineCoding))
  [Address Reference Count : 1]

  - usb_prop.o(i.Virtual_Com_Port_Data_Setup)

  Virtual_Com_Port_Status_In (Thumb, 22 bytes, Stack size 0 bytes, usb_prop.o(i.Virtual_Com_Port_Status_In))
  [Calls]

  - >> USART_Config
  [Address Reference Count : 1]
  - usb_prop.o(.data)

  Virtual_Com_Port_Status_Out (Thumb, 2 bytes, Stack size 0 bytes, usb_prop.o(i.Virtual_Com_Port_Status_Out))
  [Address Reference Count : 1]

  - usb_prop.o(.data)

  Virtual_Com_Port_init (Thumb, 34 bytes, Stack size 0 bytes, usb_prop.o(i.Virtual_Com_Port_init))
  [Calls]

  - >> USB_SIL_Init
  - >> PowerOn
  - >> USART_Config_Default
  - >> Get_SerialNum
  [Address Reference Count : 1]
  - usb_prop.o(.data)

  __0printf$1 (Thumb, 22 bytes, Stack size 0 bytes, printf1.o(i.__0printf$1), UNUSED)
  [Calls]

  - >> _printf_core

  __2printf (Thumb, 0 bytes, Stack size 0 bytes, printf1.o(i.__0printf$1))
  [Called By]

  - >> main
  - >> Count_Temperature

  fgetc (Thumb, 40 bytes, Stack size 0 bytes, usb_init.o(i.fgetc))
  [Called By]

  - >> getc

  fputc (Thumb, 66 bytes, Stack size 0 bytes, usb_init.o(i.fputc))
  [Address Reference Count : 1]

  - printf1.o(i.__0printf$1)

  getc (Thumb, 4 bytes, Stack size 0 bytes, getc.o(i.getc))
  [Calls]

  - >> fgetc
  [Called By]
  - >> main

  main (Thumb, 60 bytes, Stack size 0 bytes, main.o(i.main))
  [Calls]

  - >> getc
  - >> GPIO_ReadInputDataBit
  - >> RCC_Configuration
  - >> GPIO_Configuration
  - >> DMA_Configuration
  - >> Count_Temperature
  - >> ADC_Configuration
  - >> Set_System
  - >> __2printf
  [Address Reference Count : 1]
  - entry7.o(.ARM.Collect$$$$00000007)

  ### Local Symbols

  IntToUnicode (Thumb, 62 bytes, Stack size 0 bytes, hw_config.o(i.IntToUnicode))
  [Called By]

  - >> Get_SerialNum

  SetSysClock (Thumb, 8 bytes, Stack size 0 bytes, system_stm32f10x.o(i.SetSysClock))
  [Calls]

  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  SetSysClockTo72 (Thumb, 192 bytes, Stack size 0 bytes, system_stm32f10x.o(i.SetSysClockTo72))
  [Called By]

  - >> SetSysClock

  DataStageIn (Thumb, 172 bytes, Stack size 0 bytes, usb_core.o(i.DataStageIn))
  [Calls]

  - >> GetEPTxAddr
  - >> UserToPMABufferCopy
  - >> SetEPTxCount
  [Called By]
  - >> In0_Process
  - >> Data_Setup0

  DataStageOut (Thumb, 170 bytes, Stack size 0 bytes, usb_core.o(i.DataStageOut))
  [Calls]

  - >> PMAToUserBufferCopy
  - >> GetEPRxAddr
  - >> SetEPTxCount
  [Called By]
  - >> Out0_Process

  Data_Setup0 (Thumb, 622 bytes, Stack size 0 bytes, usb_core.o(i.Data_Setup0))
  [Calls]

  - >> DataStageIn
  [Called By]
  - >> Setup0_Process

  NoData_Setup0 (Thumb, 304 bytes, Stack size 0 bytes, usb_core.o(i.NoData_Setup0))
  [Calls]

  - >> Standard_SetInterface
  - >> Standard_SetEndPointFeature
  - >> Standard_SetDeviceFeature
  - >> Standard_SetConfiguration
  - >> Standard_ClearFeature
  [Called By]
  - >> Setup0_Process

  _printf_core (Thumb, 332 bytes, Stack size 0 bytes, printf1.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uidivmod
  [Called By]
  - >> __0printf$1

  ### Undefined Global Symbols