/**
  ******************************************************************************
  * @file    stm3210e_eval.c
  * @author  MCD Application Team
  * @version V4.2.0
  * @date    04/16/2010
  * @brief   This file provides
  *            - set of firmware functions to manage Leds, push-button and COM ports
  *            - low level initialization functions for SD card (on SDIO), SPI serial
  *              flash (sFLASH) and temperature sensor (LM75)
  *          available on STM3210E-EVAL evaluation board from STMicroelectronics.  
  ******************************************************************************
  * @copy
  *
  * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
  * TIME. AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY
  * DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING
  * FROM THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
  *
  * <h2><center>&copy; COPYRIGHT 2010 STMicroelectronics</center></h2>
  */ 
  
/* Includes ------------------------------------------------------------------*/
#include "stm3210e_eval.h"
#include "stm32f10x_spi.h"
#include "stm32f10x_i2c.h"
#include "stm32f10x_sdio.h"
#include "stm32f10x_dma.h"

/** @addtogroup Utilities
  * @{
  */ 

/** @addtogroup STM32_EVAL
  * @{
  */ 

/** @addtogroup STM3210E_EVAL
  * @{
  */ 
      
/** @defgroup STM3210E_EVAL_LOW_LEVEL 
  * @brief This file provides firmware functions to manage Leds, push-buttons, 
  *        COM ports, SD card on SDIO, serial flash (sFLASH), serial EEPROM (sEE) 
  *        and temperature sensor (LM75) available on STM3210E-EVAL evaluation 
  *        board from STMicroelectronics.
  * @{
  */ 

/** @defgroup STM3210E_EVAL_LOW_LEVEL_Private_TypesDefinitions
  * @{
  */ 
/**
  * @}
  */ 


/** @defgroup STM3210E_EVAL_LOW_LEVEL_Private_Defines
  * @{
  */ 
/**
  * @}
  */ 


/** @defgroup STM3210E_EVAL_LOW_LEVEL_Private_Macros
  * @{
  */ 
/**
  * @}
  */ 


/** @defgroup STM3210E_EVAL_LOW_LEVEL_Private_Variables
  * @{
  */ 
GPIO_TypeDef* GPIO_PORT[LEDn] = {LED1_GPIO_PORT, LED2_GPIO_PORT, LED3_GPIO_PORT,
                                 LED4_GPIO_PORT};
const uint16_t GPIO_PIN[LEDn] = {LED1_PIN, LED2_PIN, LED3_PIN,
                                 LED4_PIN};
const uint32_t GPIO_CLK[LEDn] = {LED1_GPIO_CLK, LED2_GPIO_CLK, LED3_GPIO_CLK,
                                 LED4_GPIO_CLK};

GPIO_TypeDef* BUTTON_PORT[BUTTONn] = {WAKEUP_BUTTON_GPIO_PORT, TAMPER_BUTTON_GPIO_PORT, 
                                      KEY_BUTTON_GPIO_PORT, RIGHT_BUTTON_GPIO_PORT,
                                      LEFT_BUTTON_GPIO_PORT, UP_BUTTON_GPIO_PORT,
                                      DOWN_BUTTON_GPIO_PORT, SEL_BUTTON_GPIO_PORT}; 

const uint16_t BUTTON_PIN[BUTTONn] = {WAKEUP_BUTTON_PIN, TAMPER_BUTTON_PIN, 
                                      KEY_BUTTON_PIN, RIGHT_BUTTON_PIN,
                                      LEFT_BUTTON_PIN, UP_BUTTON_PIN,
                                      DOWN_BUTTON_PIN, SEL_BUTTON_PIN}; 

const uint32_t BUTTON_CLK[BUTTONn] = {WAKEUP_BUTTON_GPIO_CLK, TAMPER_BUTTON_GPIO_CLK,
                                      KEY_BUTTON_GPIO_CLK, RIGHT_BUTTON_GPIO_CLK,
                                      LEFT_BUTTON_GPIO_CLK, UP_BUTTON_GPIO_CLK,
                                      DOWN_BUTTON_GPIO_CLK, SEL_BUTTON_GPIO_CLK};

const uint16_t BUTTON_EXTI_LINE[BUTTONn] = {WAKEUP_BUTTON_EXTI_LINE,
                                            TAMPER_BUTTON_EXTI_LINE, 
                                            KEY_BUTTON_EXTI_LINE,
                                            RIGHT_BUTTON_EXTI_LINE,
                                            LEFT_BUTTON_EXTI_LINE,
                                            UP_BUTTON_EXTI_LINE,
                                            DOWN_BUTTON_EXTI_LINE,
                                            SEL_BUTTON_EXTI_LINE};

const uint16_t BUTTON_PORT_SOURCE[BUTTONn] = {WAKEUP_BUTTON_EXTI_PORT_SOURCE,
                                              TAMPER_BUTTON_EXTI_PORT_SOURCE, 
                                              KEY_BUTTON_EXTI_PORT_SOURCE,
                                              RIGHT_BUTTON_EXTI_PORT_SOURCE,
                                              LEFT_BUTTON_EXTI_PORT_SOURCE,
                                              UP_BUTTON_EXTI_PORT_SOURCE,
                                              DOWN_BUTTON_EXTI_PORT_SOURCE,
                                              SEL_BUTTON_EXTI_PORT_SOURCE};
								 
const uint16_t BUTTON_PIN_SOURCE[BUTTONn] = {WAKEUP_BUTTON_EXTI_PIN_SOURCE,
                                             TAMPER_BUTTON_EXTI_PIN_SOURCE, 
                                             KEY_BUTTON_EXTI_PIN_SOURCE,
                                             RIGHT_BUTTON_EXTI_PIN_SOURCE,
                                             LEFT_BUTTON_EXTI_PIN_SOURCE,
                                             UP_BUTTON_EXTI_PIN_SOURCE,
                                             DOWN_BUTTON_EXTI_PIN_SOURCE,
                                             SEL_BUTTON_EXTI_PIN_SOURCE}; 

const uint16_t BUTTON_IRQn[BUTTONn] = {WAKEUP_BUTTON_EXTI_IRQn, TAMPER_BUTTON_EXTI_IRQn, 
                                       KEY_BUTTON_EXTI_IRQn, RIGHT_BUTTON_EXTI_IRQn,
                                       LEFT_BUTTON_EXTI_IRQn, UP_BUTTON_EXTI_IRQn,
                                       DOWN_BUTTON_EXTI_IRQn, SEL_BUTTON_EXTI_IRQn};

USART_TypeDef* COM_USART[COMn] = {EVAL_COM1, EVAL_COM2}; 

GPIO_TypeDef* COM_TX_PORT[COMn] = {EVAL_COM1_TX_GPIO_PORT, EVAL_COM2_TX_GPIO_PORT};
 
GPIO_TypeDef* COM_RX_PORT[COMn] = {EVAL_COM1_RX_GPIO_PORT, EVAL_COM2_RX_GPIO_PORT};
 
const uint32_t COM_USART_CLK[COMn] = {EVAL_COM1_CLK, EVAL_COM2_CLK};

const uint32_t COM_TX_PORT_CLK[COMn] = {EVAL_COM1_TX_GPIO_CLK, EVAL_COM2_TX_GPIO_CLK};
 
const uint32_t COM_RX_PORT_CLK[COMn] = {EVAL_COM1_RX_GPIO_CLK, EVAL_COM2_RX_GPIO_CLK};

const uint16_t COM_TX_PIN[COMn] = {EVAL_COM1_TX_PIN, EVAL_COM2_TX_PIN};

const uint16_t COM_RX_PIN[COMn] = {EVAL_COM1_RX_PIN, EVAL_COM2_RX_PIN};

/**
  * @}
  */ 


/** @defgroup STM3210E_EVAL_LOW_LEVEL_Private_FunctionPrototypes
  * @{
  */ 

/**
  * @}
  */ 


/** @defgroup STM3210E_EVAL_LOW_LEVEL_Private_Functions
  * @{
  */ 

/**
  * @brief  Configures LED GPIO.
  * @param  Led: Specifies the Led to be configured. 
  *   This parameter can be one of following parameters:
  *     @arg LED1
  *     @arg LED2
  *     @arg LED3
  *     @arg LED4
  * @retval None
  */
void STM_EVAL_LEDInit(Led_TypeDef Led)
{
  GPIO_InitTypeDef  GPIO_InitStructure;
  
  /* Enable the GPIO_LED Clock */
  RCC_APB2PeriphClockCmd(GPIO_CLK[Led], ENABLE);

  /* Configure the GPIO_LED pin */
  GPIO_InitStructure.GPIO_Pin = GPIO_PIN[Led];
  GPIO_InitStructure.GPIO_Mode = GPIO_Mode_Out_PP;
  GPIO_InitStructure.GPIO_Speed = GPIO_Speed_50MHz;

  GPIO_Init(GPIO_PORT[Led], &GPIO_InitStructure);
}

/**
  * @brief  Turns selected LED On.
  * @param  Led: Specifies the Led to be set on. 
  *   This parameter can be one of following parameters:
  *     @arg LED1
  *     @arg LED2
  *     @arg LED3
  *     @arg LED4  
  * @retval None
  */
void STM_EVAL_LEDOn(Led_TypeDef Led)
{
  GPIO_PORT[Led]->BSRR = GPIO_PIN[Led];     
}

/**
  * @brief  Turns selected LED Off.
  * @param  Led: Specifies the Led to be set off. 
  *   This parameter can be one of following parameters:
  *     @arg LED1
  *     @arg LED2
  *     @arg LED3
  *     @arg LED4 
  * @retval None
  */
void STM_EVAL_LEDOff(Led_TypeDef Led)
{
  GPIO_PORT[Led]->BRR = GPIO_PIN[Led];    
}

/**
  * @brief  Toggles the selected LED.
  * @param  Led: Specifies the Led to be toggled. 
  *   This parameter can be one of following parameters:
  *     @arg LED1
  *     @arg LED2
  *     @arg LED3
  *     @arg LED4  
  * @retval None
  */
void STM_EVAL_LEDToggle(Led_TypeDef Led)
{
  GPIO_PORT[Led]->ODR ^= GPIO_PIN[Led];
}

/**
  * @brief  Configures Button GPIO and EXTI Line.
  * @param  Button: Specifies the Button to be configured.
  *   This parameter can be one of following parameters:   
  *     @arg BUTTON_WAKEUP: Wakeup Push Button
  *     @arg BUTTON_TAMPER: Tamper Push Button  
  *     @arg BUTTON_KEY: Key Push Button 
  *     @arg BUTTON_RIGHT: Joystick Right Push Button 
  *     @arg BUTTON_LEFT: Joystick Left Push Button 
  *     @arg BUTTON_UP: Joystick Up Push Button 
  *     @arg BUTTON_DOWN: Joystick Down Push Button
  *     @arg BUTTON_SEL: Joystick Sel Push Button
  * @param  Button_Mode: Specifies Button mode.
  *   This parameter can be one of following parameters:   
  *     @arg BUTTON_MODE_GPIO: Button will be used as simple IO 
  *     @arg BUTTON_MODE_EXTI: Button will be connected to EXTI line with interrupt
  *                     generation capability  
  * @retval None
  */
void STM_EVAL_PBInit(Button_TypeDef Button, ButtonMode_TypeDef Button_Mode)
{
  GPIO_InitTypeDef GPIO_InitStructure;
  EXTI_InitTypeDef EXTI_InitStructure;
  NVIC_InitTypeDef NVIC_InitStructure;

  /* Enable the BUTTON Clock */
  RCC_APB2PeriphClockCmd(BUTTON_CLK[Button] | RCC_APB2Periph_AFIO, ENABLE);

  /* Configure Button pin as input floating */
  GPIO_InitStructure.GPIO_Mode = GPIO_Mode_IN_FLOATING;
  GPIO_InitStructure.GPIO_Pin = BUTTON_PIN[Button];
  GPIO_Init(BUTTON_PORT[Button], &GPIO_InitStructure);


  if (Button_Mode == BUTTON_MODE_EXTI)
  {
    /* Connect Button EXTI Line to Button GPIO Pin */
    GPIO_EXTILineConfig(BUTTON_PORT_SOURCE[Button], BUTTON_PIN_SOURCE[Button]);

    /* Configure Button EXTI line */
    EXTI_InitStructure.EXTI_Line = BUTTON_EXTI_LINE[Button];
    EXTI_InitStructure.EXTI_Mode = EXTI_Mode_Interrupt;

    if(Button != BUTTON_WAKEUP)
    {
      EXTI_InitStructure.EXTI_Trigger = EXTI_Trigger_Falling;  
    }
    else
    {
      EXTI_InitStructure.EXTI_Trigger = EXTI_Trigger_Rising;  
    }
    EXTI_InitStructure.EXTI_LineCmd = ENABLE;
    EXTI_Init(&EXTI_InitStructure);

    /* Enable and set Button EXTI Interrupt to the lowest priority */
    NVIC_InitStructure.NVIC_IRQChannel = BUTTON_IRQn[Button];
    NVIC_InitStructure.NVIC_IRQChannelPreemptionPriority = 0x0F;
    NVIC_InitStructure.NVIC_IRQChannelSubPriority = 0x0F;
    NVIC_InitStructure.NVIC_IRQChannelCmd = ENABLE;

    NVIC_Init(&NVIC_InitStructure); 
  }
}

/**
  * @brief  Returns the selected Button state.
  * @param  Button: Specifies the Button to be checked.
  *   This parameter can be one of following parameters:    
  *     @arg BUTTON_WAKEUP: Wakeup Push Button
  *     @arg BUTTON_TAMPER: Tamper Push Button  
  *     @arg BUTTON_KEY: Key Push Button 
  *     @arg BUTTON_RIGHT: Joystick Right Push Button 
  *     @arg BUTTON_LEFT: Joystick Left Push Button 
  *     @arg BUTTON_UP: Joystick Up Push Button 
  *     @arg BUTTON_DOWN: Joystick Down Push Button
  *     @arg BUTTON_SEL: Joystick Sel Push Button    
  * @retval The Button GPIO pin value.
  */
uint32_t STM_EVAL_PBGetState(Button_TypeDef Button)
{
  return GPIO_ReadInputDataBit(BUTTON_PORT[Button], BUTTON_PIN[Button]);
}

/**
  * @brief  Configures COM port.
  * @param  COM: Specifies the COM port to be configured.
  *   This parameter can be one of following parameters:    
  *     @arg COM1
  *     @arg COM2  
  * @param  USART_InitStruct: pointer to a USART_InitTypeDef structure that
  *   contains the configuration information for the specified USART peripheral.
  * @retval None
  */
void STM_EVAL_COMInit(COM_TypeDef COM, USART_InitTypeDef* USART_InitStruct)
{
  GPIO_InitTypeDef GPIO_InitStructure;

  /* Enable GPIO clock */
  RCC_APB2PeriphClockCmd(COM_TX_PORT_CLK[COM] | COM_RX_PORT_CLK[COM] | RCC_APB2Periph_AFIO, ENABLE);

  /* Enable UART clock */
  if (COM == COM1)
  {
    RCC_APB2PeriphClockCmd(COM_USART_CLK[COM], ENABLE); 
  }
  else
  {
    RCC_APB1PeriphClockCmd(COM_USART_CLK[COM], ENABLE);
  }

  /* Configure USART Tx as alternate function push-pull */
  GPIO_InitStructure.GPIO_Mode = GPIO_Mode_AF_PP;
  GPIO_InitStructure.GPIO_Pin = COM_TX_PIN[COM];
  GPIO_InitStructure.GPIO_Speed = GPIO_Speed_50MHz;
  GPIO_Init(COM_TX_PORT[COM], &GPIO_InitStructure);

  /* Configure USART Rx as input floating */
  GPIO_InitStructure.GPIO_Mode = GPIO_Mode_IN_FLOATING;
  GPIO_InitStructure.GPIO_Pin = COM_RX_PIN[COM];
  GPIO_Init(COM_RX_PORT[COM], &GPIO_InitStructure);

  /* USART configuration */
  USART_Init(COM_USART[COM], USART_InitStruct);
    
  /* Enable USART */
  USART_Cmd(COM_USART[COM], ENABLE);
}

/**
  * @brief  DeInitializes the SDIO interface.
  * @param  None
  * @retval None
  */
void SD_LowLevel_DeInit(void)
{
  GPIO_InitTypeDef  GPIO_InitStructure;
  
  /*!< Disable SDIO Clock */
  SDIO_ClockCmd(DISABLE);
  
  /*!< Set Power State to OFF */
  SDIO_SetPowerState(SDIO_PowerState_OFF);

  /*!< DeInitializes the SDIO peripheral */
  SDIO_DeInit();
  
  /*!< Disable the SDIO AHB Clock */
  RCC_AHBPeriphClockCmd(RCC_AHBPeriph_SDIO, DISABLE);

  /*!< Configure PC.08, PC.09, PC.10, PC.11, PC.12 pin: D0, D1, D2, D3, CLK pin */
  GPIO_InitStructure.GPIO_Pin = GPIO_Pin_8 | GPIO_Pin_9 | GPIO_Pin_10 | GPIO_Pin_11 | GPIO_Pin_12;
  GPIO_InitStructure.GPIO_Mode = GPIO_Mode_IN_FLOATING;
  GPIO_Init(GPIOC, &GPIO_InitStructure);

  /*!< Configure PD.02 CMD line */
  GPIO_InitStructure.GPIO_Pin = GPIO_Pin_2;
  GPIO_Init(GPIOD, &GPIO_InitStructure);
}

/**
  * @brief  Initializes the SD Card and put it into StandBy State (Ready for 
  *         data transfer).
  * @param  None
  * @retval None
  */
void SD_LowLevel_Init(void)
{
  GPIO_InitTypeDef  GPIO_InitStructure;

  /*!< GPIOC and GPIOD Periph clock enable */
  RCC_APB2PeriphClockCmd(RCC_APB2Periph_GPIOC | RCC_APB2Periph_GPIOD | SD_DETECT_GPIO_CLK, ENABLE);

  /*!< Configure PC.08, PC.09, PC.10, PC.11, PC.12 pin: D0, D1, D2, D3, CLK pin */
  GPIO_InitStructure.GPIO_Pin = GPIO_Pin_8 | GPIO_Pin_9 | GPIO_Pin_10 | GPIO_Pin_11 | GPIO_Pin_12;
  GPIO_InitStructure.GPIO_Speed = GPIO_Speed_50MHz;
  GPIO_InitStructure.GPIO_Mode = GPIO_Mode_AF_PP;
  GPIO_Init(GPIOC, &GPIO_InitStructure);

  /*!< Configure PD.02 CMD line */
  GPIO_InitStructure.GPIO_Pin = GPIO_Pin_2;
  GPIO_Init(GPIOD, &GPIO_InitStructure);

  /*!< Configure SD_SPI_DETECT_PIN pin: SD Card detect pin */
  GPIO_InitStructure.GPIO_Pin = SD_DETECT_PIN;
  GPIO_InitStructure.GPIO_Mode = GPIO_Mode_IPU;
  GPIO_Init(SD_DETECT_GPIO_PORT, &GPIO_InitStructure);
  
  /*!< Enable the SDIO AHB Clock */
  RCC_AHBPeriphClockCmd(RCC_AHBPeriph_SDIO, ENABLE);

  /*!< Enable the DMA2 Clock */
  RCC_AHBPeriphClockCmd(RCC_AHBPeriph_DMA2, ENABLE);
}

/**
  * @brief  Configures the DMA2 Channel4 for SDIO Tx request.
  * @param  BufferSRC: pointer to the source buffer
  * @param  BufferSize: buffer size
  * @retval None
  */
void SD_LowLevel_DMA_TxConfig(uint32_t *BufferSRC, uint32_t BufferSize)
{

  DMA_InitTypeDef DMA_InitStructure;

  DMA_ClearFlag(DMA2_FLAG_TC4 | DMA2_FLAG_TE4 | DMA2_FLAG_HT4 | DMA2_FLAG_GL4);

  /*!< DMA2 Channel4 disable */
  DMA_Cmd(DMA2_Channel4, DISABLE);

  /*!< DMA2 Channel4 Config */
  DMA_InitStructure.DMA_PeripheralBaseAddr = (uint32_t)SDIO_FIFO_ADDRESS;
  DMA_InitStructure.DMA_MemoryBaseAddr = (uint32_t)BufferSRC;
  DMA_InitStructure.DMA_DIR = DMA_DIR_PeripheralDST;
  DMA_InitStructure.DMA_BufferSize = BufferSize / 4;
  DMA_InitStructure.DMA_PeripheralInc = DMA_PeripheralInc_Disable;
  DMA_InitStructure.DMA_MemoryInc = DMA_MemoryInc_Enable;
  DMA_InitStructure.DMA_PeripheralDataSize = DMA_PeripheralDataSize_Word;
  DMA_InitStructure.DMA_MemoryDataSize = DMA_MemoryDataSize_Word;
  DMA_InitStructure.DMA_Mode = DMA_Mode_Normal;
  DMA_InitStructure.DMA_Priority = DMA_Priority_High;
  DMA_InitStructure.DMA_M2M = DMA_M2M_Disable;
  DMA_Init(DMA2_Channel4, &DMA_InitStructure);

  /*!< DMA2 Channel4 enable */
  DMA_Cmd(DMA2_Channel4, ENABLE);  
}

/**
  * @brief  Configures the DMA2 Channel4 for SDIO Rx request.
  * @param  BufferDST: pointer to the destination buffer
  * @param  BufferSize: buffer size
  * @retval None
  */
void SD_LowLevel_DMA_RxConfig(uint32_t *BufferDST, uint32_t BufferSize)
{
  DMA_InitTypeDef DMA_InitStructure;

  DMA_ClearFlag(DMA2_FLAG_TC4 | DMA2_FLAG_TE4 | DMA2_FLAG_HT4 | DMA2_FLAG_GL4);

  /*!< DMA2 Channel4 disable */
  DMA_Cmd(DMA2_Channel4, DISABLE);

  /*!< DMA2 Channel4 Config */
  DMA_InitStructure.DMA_PeripheralBaseAddr = (uint32_t)SDIO_FIFO_ADDRESS;
  DMA_InitStructure.DMA_MemoryBaseAddr = (uint32_t)BufferDST;
  DMA_InitStructure.DMA_DIR = DMA_DIR_PeripheralSRC;
  DMA_InitStructure.DMA_BufferSize = BufferSize / 4;
  DMA_InitStructure.DMA_PeripheralInc = DMA_PeripheralInc_Disable;
  DMA_InitStructure.DMA_MemoryInc = DMA_MemoryInc_Enable;
  DMA_InitStructure.DMA_PeripheralDataSize = DMA_PeripheralDataSize_Word;
  DMA_InitStructure.DMA_MemoryDataSize = DMA_MemoryDataSize_Word;
  DMA_InitStructure.DMA_Mode = DMA_Mode_Normal;
  DMA_InitStructure.DMA_Priority = DMA_Priority_High;
  DMA_InitStructure.DMA_M2M = DMA_M2M_Disable;
  DMA_Init(DMA2_Channel4, &DMA_InitStructure);

  /*!< DMA2 Channel4 enable */
  DMA_Cmd(DMA2_Channel4, ENABLE); 
}

/**
  * @brief  Wait For DMA End Of Transfer.
  * @param  None
  * @retval None
  */
void SD_WaitForDMAEndOfTransfer(void)
{
  while (DMA_GetFlagStatus(DMA2_FLAG_TC4) == RESET)
  {}
}

/**
  * @brief  DeInitializes the peripherals used by the SPI FLASH driver.
  * @param  None
  * @retval None
  */
void sFLASH_LowLevel_DeInit(void)
{
  GPIO_InitTypeDef GPIO_InitStructure;

  /*!< Disable the sFLASH_SPI  */
  SPI_Cmd(sFLASH_SPI, DISABLE);
  
  /*!< DeInitializes the sFLASH_SPI */
  SPI_I2S_DeInit(sFLASH_SPI);
  
  /*!< sFLASH_SPI Periph clock disable */
  RCC_APB2PeriphClockCmd(sFLASH_SPI_CLK, DISABLE);
  
  /*!< Configure sFLASH_SPI pins: SCK */
  GPIO_InitStructure.GPIO_Pin = sFLASH_SPI_SCK_PIN;
  GPIO_InitStructure.GPIO_Mode = GPIO_Mode_IN_FLOATING;
  GPIO_Init(sFLASH_SPI_SCK_GPIO_PORT, &GPIO_InitStructure);

  /*!< Configure sFLASH_SPI pins: MISO */
  GPIO_InitStructure.GPIO_Pin = sFLASH_SPI_MISO_PIN;
  GPIO_Init(sFLASH_SPI_MISO_GPIO_PORT, &GPIO_InitStructure);

  /*!< Configure sFLASH_SPI pins: MOSI */
  GPIO_InitStructure.GPIO_Pin = sFLASH_SPI_MOSI_PIN;
  GPIO_Init(sFLASH_SPI_MOSI_GPIO_PORT, &GPIO_InitStructure);

  /*!< Configure sFLASH_CS_PIN pin: sFLASH Card CS pin */
  GPIO_InitStructure.GPIO_Pin = sFLASH_CS_PIN;
  GPIO_Init(sFLASH_CS_GPIO_PORT, &GPIO_InitStructure);
}

/**
  * @brief  Initializes the peripherals used by the SPI FLASH driver.
  * @param  None
  * @retval None
  */
void sFLASH_LowLevel_Init(void)
{
  GPIO_InitTypeDef GPIO_InitStructure;

  /*!< sFLASH_SPI_CS_GPIO, sFLASH_SPI_MOSI_GPIO, sFLASH_SPI_MISO_GPIO 
       and sFLASH_SPI_SCK_GPIO Periph clock enable */
  RCC_APB2PeriphClockCmd(sFLASH_CS_GPIO_CLK | sFLASH_SPI_MOSI_GPIO_CLK | sFLASH_SPI_MISO_GPIO_CLK |
                         sFLASH_SPI_SCK_GPIO_CLK, ENABLE);

  /*!< sFLASH_SPI Periph clock enable */
  RCC_APB2PeriphClockCmd(sFLASH_SPI_CLK, ENABLE);
  
  /*!< Configure sFLASH_SPI pins: SCK */
  GPIO_InitStructure.GPIO_Pin = sFLASH_SPI_SCK_PIN;
  GPIO_InitStructure.GPIO_Speed = GPIO_Speed_50MHz;
  GPIO_InitStructure.GPIO_Mode = GPIO_Mode_AF_PP;
  GPIO_Init(sFLASH_SPI_SCK_GPIO_PORT, &GPIO_InitStructure);

  /*!< Configure sFLASH_SPI pins: MISO */
  GPIO_InitStructure.GPIO_Pin = sFLASH_SPI_MISO_PIN;
  GPIO_Init(sFLASH_SPI_MISO_GPIO_PORT, &GPIO_InitStructure);

  /*!< Configure sFLASH_SPI pins: MOSI */
  GPIO_InitStructure.GPIO_Pin = sFLASH_SPI_MOSI_PIN;
  GPIO_Init(sFLASH_SPI_MOSI_GPIO_PORT, &GPIO_InitStructure);

  /*!< Configure sFLASH_CS_PIN pin: sFLASH Card CS pin */
  GPIO_InitStructure.GPIO_Pin = sFLASH_CS_PIN;
  GPIO_InitStructure.GPIO_Mode = GPIO_Mode_Out_PP;
  GPIO_Init(sFLASH_CS_GPIO_PORT, &GPIO_InitStructure);
}

/**
  * @brief  DeInitializes the LM75_I2C.
  * @param  None
  * @retval None
  */
void LM75_LowLevel_DeInit(void)
{
  GPIO_InitTypeDef  GPIO_InitStructure;

  /*!< Disable LM75_I2C */
  I2C_Cmd(LM75_I2C, DISABLE);
  /*!< DeInitializes the LM75_I2C */
  I2C_DeInit(LM75_I2C);
  
  /*!< LM75_I2C Periph clock disable */
  RCC_APB1PeriphClockCmd(LM75_I2C_CLK, DISABLE);
    
  /*!< Configure LM75_I2C pins: SCL */
  GPIO_InitStructure.GPIO_Pin = LM75_I2C_SCL_PIN;
  GPIO_InitStructure.GPIO_Mode = GPIO_Mode_IN_FLOATING;
  GPIO_Init(LM75_I2C_SCL_GPIO_PORT, &GPIO_InitStructure);

  /*!< Configure LM75_I2C pins: SDA */
  GPIO_InitStructure.GPIO_Pin = LM75_I2C_SDA_PIN;
  GPIO_Init(LM75_I2C_SDA_GPIO_PORT, &GPIO_InitStructure);

  /*!< Configure LM75_I2C pin: SMBUS ALERT */
  GPIO_InitStructure.GPIO_Pin = LM75_I2C_SMBUSALERT_PIN;
  GPIO_Init(LM75_I2C_SMBUSALERT_GPIO_PORT, &GPIO_InitStructure);
}

/**
  * @brief  Initializes the LM75_I2C..
  * @param  None
  * @retval None
  */
void LM75_LowLevel_Init(void)
{
  GPIO_InitTypeDef  GPIO_InitStructure;

  /*!< LM75_I2C Periph clock enable */
  RCC_APB1PeriphClockCmd(LM75_I2C_CLK, ENABLE);
    
  /*!< LM75_I2C_SCL_GPIO_CLK, LM75_I2C_SDA_GPIO_CLK 
       and LM75_I2C_SMBUSALERT_GPIO_CLK Periph clock enable */
  RCC_APB2PeriphClockCmd(LM75_I2C_SCL_GPIO_CLK | LM75_I2C_SDA_GPIO_CLK |
                         LM75_I2C_SMBUSALERT_GPIO_CLK, ENABLE);
  
  /*!< Configure LM75_I2C pins: SCL */
  GPIO_InitStructure.GPIO_Pin = LM75_I2C_SCL_PIN;
  GPIO_InitStructure.GPIO_Speed = GPIO_Speed_50MHz;
  GPIO_InitStructure.GPIO_Mode = GPIO_Mode_AF_OD;
  GPIO_Init(LM75_I2C_SCL_GPIO_PORT, &GPIO_InitStructure);

  /*!< Configure LM75_I2C pins: SDA */
  GPIO_InitStructure.GPIO_Pin = LM75_I2C_SDA_PIN;
  GPIO_Init(LM75_I2C_SDA_GPIO_PORT, &GPIO_InitStructure);

  /*!< Configure LM75_I2C pin: SMBUS ALERT */
  GPIO_InitStructure.GPIO_Pin = LM75_I2C_SMBUSALERT_PIN;
  GPIO_InitStructure.GPIO_Mode = GPIO_Mode_IPU;
  GPIO_Init(LM75_I2C_SMBUSALERT_GPIO_PORT, &GPIO_InitStructure); 
}

/**
  * @}
  */ 

/**
  * @}
  */ 

/**
  * @}
  */

/**
  * @}
  */    

/**
  * @}
  */ 
    
/******************* (C) COPYRIGHT 2010 STMicroelectronics *****END OF FILE****/
